Z8E version 4.0
===============

This update incorporates the HD64180/Z180 extensions developed by Damon
Gibson as well those to enable a secondary terminal attached to the AUX
device.

There is no attempt to maintain binary patch capability.  It is assumed
that anyone running Z8E/18E will have access to at least one of the Z80
assemblers needed to build the program.

I have noticed an issue which interferes with loading a symbol table from
a .PRN or .LST file.  It seems to occur when the sentinel text identfying
the start of the table spans a sector boundary.  I have not tracked down
the cause yet.  It will be included in a later release.

The documentation has not changed and is not inclued in this volume.  It
can be found on volume 85 of this collection inside Z8E36.ARC.

A CP/M 3 submit file is supplied for Z80ASM.  It generates four versions
of Z8E:

	18E1.COM	Z180 support, one terminal
	18E2.COM	Z180 support, two terminals
	Z8E1.COM	Z80, one terminal ("standard" version)
	Z8E2.COM	Z80, two terminals

Note that on the two-terminal versions, the program being debugged writes
to the main terminal (CON:) and the debugger uses the second (AUX:)
terminal.

Jon Saxton
tesseract@triton.vg

